{"text_format":"3","workbook":"xls","n_sheets":6,"sheets":["Change_History","Sheet_Info","video_atop","demod_atop","dvi_atop","dvi_top_oneport"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Change_History","index":0,"n_rows":9,"n_cols":3,"rows_kept":9,"flags":["formulas_cached_only"]}
["Version","Date","Description"]
["0.0","2010/03/22","first collection"]
["0.1","2010/04/14","1. remove saradc/mod/ddr/audio/usb sheet\n2. change sheet_info sheet"]
["0.2","2010/04/16","python script gen OK"]
["0.3","2010/04/16","modify DVI address"]
["0.4","2010/05/19","Disable DVI_atop/DVI_TOP_ONEPORT"]
["0.5","2010-06-23","Add Video PHD on/off control"]
["0.6","2010/07/01","update video_atop PD_REF_RGB/PD_REF_YUV"]
["0.7","2010/07/01","turn on PD_REF_YUV at SCART MODE & renamefile to v0.6"]

{"sheet":"Sheet_Info","index":1,"n_rows":18,"n_cols":4,"rows_kept":18,"flags":["formulas_cached_only"]}
["IP list 總表(mapping tbl)","PWS src\n//此內容與IP list所填寫的內容是對應的\n//由designer填寫","Input source Mapping table\nfor 將PWS src 與外層\"應用程式\"的Input source對照\n//此欄位的值與右側的Input source reference一致\n//由designer填寫","maxinum input source list\n//for Mapping table填寫參考使用, \n//不會變動\n//若此list找不到需要的Input source, 就要Highlight出來, 找撰寫外層\"應用程式\"的同仁一起討論了"]
["Sheet list:","Use case","Input source for AP use","Input source reference"]
["video_atop","CVBSO-I","CVBSO-I","CVBSO-I"]
["demod_atop","CVBSO-E","CVBSO-E","CVBSO-E"]
["dvi_atop","DTV-DVB","DTV-DVB","DTV-DVB"]
["dvi_top_oneport","DTV-ATSC","DTV-ATSC","DTV-ATSC"]
[null,"ATV-VIF","ATV-VIF","ATV-VIF"]
[null,"ATV-SSIF","ATV-SSIF","ATV-SSIF"]
[null,"CVBS","CVBS","CVBS"]
[null,"RGB","RGB","RGB"]
[null,"SCART","SCART","SCART"]
[null,"YPbPr","YPbPr","YPbPr"]
[null,"HDMI1","HDMI1","HDMI1"]
[null,"HDMI2","HDMI2","HDMI2"]
[null,"HDMI3","HDMI3","HDMI3"]
[null,"HDMI4","HDMI4","HDMI4"]
[null,"S-Video","S-Video","S-Video"]
[null,"USB","USB","USB"]

{"sheet":"video_atop","index":2,"n_rows":49,"n_cols":26,"rows_kept":49,"merged":[[2,0,48,0],[12,22,16,22],[12,23,16,23],[12,24,16,24]],"flags":["formulas_cached_only"]}
["1.表格依照開關順序排列\n2.需要delay的部分視為一個項目, python可由address來判斷該項目是否為delay\n3.SYNC_DETECT (off-line Detect)暫時未考慮",null,"統一8bits",null,"此欄位表示該reg On/off開關\n與其他reg的設定剛好相反\nex: \n一般ON=0x00, OFF=0x01, Invert =N\n特別ON=0x01, OFF=0x00, Invert =Y","SW Debug use\nY= 要設定\nN= 不設定","ATV in \n(use internal demod)","ATV in \n(use external demod)",{"$nulls":14},"SW/CAE參考","SW/CAE參考"]
[null,"Reg Name","Address","Mask","Invert","Valid","CVBSO-I","CVBSO-E","DTV-DVB","DTV-ATSC","ATV-VIF","ATV-SSIF","CVBS","RGB","SCART","YPbPr","HDMI1","HDMI2","HDMI3","HDMI4","S-Video","USB","1.0V","2.5V","3.3V","description"]
[null,"EN_MUX_RGB","0x102503","0x40","Y","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF",0,0,0,"RGB_MUX Enable"]
[null,"PD_ICLP_RGB","0x102509","0x04","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF",0.05,0.001,0.002,"RGB I-clamp power down"]
[null,"PD_ICLP_VDY","0x102509","0x08","N","Y","OFF","ON","OFF","OFF","OFF","ON","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","ON","OFF",0.05,0.001,0.002,"VDY I-clamp power down"]
[null,"PD_ICLP_VDC","0x102509","0x10","N","Y","OFF","ON","OFF","OFF","OFF","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF",0.05,0.001,0.002,"VDC I-clamp power down"]
[null,"PD_SOG_DAC","0x10250a","0x04","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",0,0.03,0,"SOG_DAC power down"]
[null,"PD_SOG_MAIN","0x10250A","0x08","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",0,0.07,0,"SOG power down"]
[null,"PD_SOG_MUX","0x10257E","0x01","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",0,0,0,"SOG MUX power down"]
[null,"PD_SOGOFF_DAC","0x10250A","0x10","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",0,0.03,0,"SOG_DAC power down (off-line)"]
[null,"PD_SOGOFF_MAIN","0x10250A","0x20","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",0,0.07,0,"SOG power down (off-line)"]
[null,"PD_SOGOFF_MUX","0x10257e","0x02","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",0,0,0,"SOG MUX power down (off-line)"]
[null,"PD_BG","0x102508","0x04","N","Y","ON","ON","OFF","OFF","OFF","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","ON","OFF",0,1.5,0,"Band-gap power down"]
[null,"PD_REF","0x102508","0x08","N","Y","ON","ON","OFF","OFF","OFF","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","ON","OFF",{"$nulls":3},"REF system power down"]
[null,"PD_REF_RGB","0x102508","0x01","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","ON","ON","OFF","OFF","OFF","OFF","ON","OFF",{"$nulls":3},"RGB ADC reference power down"]
[null,"PD_REF_VD","0x102508","0x02","N","Y","OFF","ON","OFF","OFF","OFF","ON","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","ON","OFF",{"$nulls":3},"VD ADC reference power down"]
[null,"PD_REF_YUV","0x102508","0x10","N","Y","OFF","ON","OFF","OFF","OFF","ON","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","ON","OFF",{"$nulls":3},"YUV ADC reference power down"]
[null,"EN_MUX_VD_Y","0x102505","0x01","Y","Y","OFF","ON","OFF","OFF","OFF","ON","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","ON","OFF",0,0,0,"VD_Y_MUX Enable"]
[null,"EN_MUX_VD_C","0x102505","0x02","Y","Y","OFF","ON","OFF","OFF","OFF","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF",0,0,0,"VD_C_MUX Enable"]
[null,"EN_VDLPF_C","0x102570","0x02","Y","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF",0.05,1.3,1.4,"VD_LPF_C Enable"]
[null,"EN_VDLPF_Y","0x102570","0x01","Y","Y","OFF","ON","OFF","OFF","OFF","ON","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","ON","OFF",0.05,1.3,1.4,"VD_LPF_C Enable"]
[null,"EN_IDAC1","0x102590","0x08","Y","Y","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",0.05,0,10,"CVBS_DAC_1 Enable"]
[null,"EN_IDAC_REF","0x103d00","0x10","Y","Y","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",0.05,0,10,"CVBS_DAC_1 Enable"]
[null,"EN_IDAC_PLUGOET","0x103d0A","0x10","Y","Y","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",0.05,0,10,"Enable Channel X plug detection Enable"]
[null,"EN_IDAC2","0x102592","0x08","Y","Y","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",0.05,0,10,"CVBS_DAC_2 Enable"]
[null,"PD_HSYNC0_COMP","0x10250b","0x01","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",0,0.5,0,"HSYNC comperator 0 Enable"]
[null,"PD_HSYNC1_COMP","0x10250b","0x02","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",0,0.5,0,"HSYNC comperator 1 Enable"]
[null,"PD_HSYNC2_COMP","0x10250b","0x04","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",0,0.5,0,"HSYNC comperator 2 Enable"]
[null,"PD_ADCPLA_REG","0x102509","0x02","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",0,10,0,"ADCPLL_A power down"]
[null,"PD_ADCPLB_REG","0x10250A","0x02","N","Y","OFF","ON","OFF","OFF","OFF","ON","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","ON","OFF",0,10,0,"ADCPLL_B power down"]
[null,"GCR_PGDIG_D_PD","0x10250B","0x08","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",0,1,0,"digital PHD power down"]
[null,"PD_PGDIG_A","0x102509","0x01","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",0,1.23,0,"analog PHD power down"]
[null,"PD_ADCR","0x102508","0x20","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","ON","ON","OFF","OFF","OFF","OFF","ON","OFF",1.2,20,1.5,"ADC R power down"]
[null,"PD_ADCG","0x102508","0x40","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF",1.2,20,1.5,"ADC G power down"]
[null,"PD_ADCB","0x102508","0x80","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF",1.2,20,1.5,"ADC B power down"]
[null,"PD_ADCY","0x102509","0x40","N","Y","OFF","ON","OFF","OFF","OFF","ON","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","ON","OFF",1.2,20,1.5,"ADC Y power down"]
[null,"PD_FBLANK","0x102580","0x40","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF",0.5,1,0,"Fast Blank ADC power down"]
[null,"PD_ADCA_PHDAC_R","0x1025BC","0x40","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",{"$nulls":3},"ADCPLA Phase Dac R power down"]
[null,"PD_ADCA_PHDAC_G","0x1025BC","0x80","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",{"$nulls":3},"ADCPLA Phase Dac G power down"]
[null,"PD_ADCA_PHDAC_B","0x1025BD","0x01","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF",{"$nulls":3},"ADCPLA Phase Dac B power down"]
[null,"PD_ADCA_PHDAC_Y","0x1025BD","0x02","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",{"$nulls":3},"ADCPLA Phase Dac Y power down"]
[null,"PD_ADCB_PHDAC_R","0x1025BD","0x04","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF","ON","OFF",{"$nulls":3},"ADCPLB Phase Dac R power down"]
[null,"PD_ADCB_PHDAC_G","0x1025BD","0x08","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF",{"$nulls":3},"ADCPLB Phase Dac G power down"]
[null,"PD_ADCB_PHDAC_B","0x1025BD","0x10","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF",{"$nulls":3},"ADCPLB Phase Dac B power down"]
[null,"PD_ADCB_PHDAC_Y","0x1025BD","0x20","N","Y","OFF","ON","OFF","OFF","OFF","ON","ON","OFF","ON","OFF","OFF","OFF","OFF","OFF","ON","OFF",{"$nulls":3},"ADCPLB Phase Dac Y power down"]
[null,"reg_pd_ldo","0x1025B4","0x20","N","Y","ON","ON","OFF","OFF","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","ON","OFF"]
[null,"reg_pd_ldo25_adca","0x1025B4","0x40","N","Y","ON","ON","OFF","OFF","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","ON","OFF"]
[null,"reg_pd_ldo25_adcb","0x1025B4","0x80","N","Y","ON","ON","OFF","OFF","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","ON","OFF"]
[null,"REG_LDO","0x102561","0x01","N","Y","ON","ON","OFF","OFF","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","ON","OFF"]

{"sheet":"demod_atop","index":3,"n_rows":17,"n_cols":24,"rows_kept":17,"merged":[[2,0,16,0]],"flags":["formulas_cached_only"]}
["1.表格依照開關順序排列\n2.需要delay的部分視為一個項目, python可由address來判斷該項目是否為delay\n3.SYNC_DETECT (off-line Detect)暫時未考慮",null,"統一8bits",null,"此欄位表示該reg On/off開關\n與其他reg的設定剛好相反\nex: \n一般ON=0x00, OFF=0x01, Invert =N\n特別ON=0x01, OFF=0x00, Invert =Y","SW Debug use\nY= 要設定\nN= 不設定","ATV in \n(use internal demod)","ATV in \n(use external demod)",{"$nulls":14},"SW/CAE參考","SW/CAE參考"]
[null,"Reg Name","Address","Mask","Invert","Valid","CVBSO-I","CVBSO-E","DTV-DVB","DTV-ATSC","ATV-VIF","ATV-SSIF","CVBS","RGB","SCART","YPbPr","HDMI1","HDMI2","HDMI3","HDMI4","S-Video","USB","Power consumption","Description"]
["Demod_atop","PWDN_REF","0x112840","0x10","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Powerdown ADC reference voltage"]
[null,"PWDN_CLPBUF","0x112818","0x04","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Powerdown clamp buffer"]
[null,"PWDN_VCALBUF","0x11281E","0x80","N","Y","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Powerdown calibration buffer"]
[null,"PWDN_ADC","0x112818","0x01","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Powerdown ADC I"]
[null,"DMLDO_PD","0x112879","0x10","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Powerdown 2.5V LDO"]
[null,"MPLL_PD","0x11286A","0x80","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Powerdown MPLL"]
[null,"PD_DMPLL_CLK","0x11286B","0x20","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Power down demod PLL's ref clock"]
[null,"MPLL_ADC_CLK_PD","0x112860","0x02","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Power down demod_ADC's clock"]
[null,"MPLL_DIV2_PD","0x112860","0x04","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Digital divider (/2) power down "]
[null,"MPLL_DIV3_PD","0x112860","0x08","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Digital divider (/3) power down "]
[null,"MPLL_DIV4_PD","0x112860","0x10","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Digital divider (/4) power down "]
[null,"MPLL_DIV8_PD","0x112860","0x20","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Digital divider (/8) power down "]
[null,"MPLL_DIV10_PD","0x112860","0x40","N","Y","ON","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Digital divider (/10) power down "]
[null,"IFAGC_PWR","0x11286C","0x10","Y","Y","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Enable IFAGC"]
[null,"RFAGC_PWR","0x11286C","0x01","Y","Y","ON","ON","ON","ON","ON","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF",null,"Enable IFAGC"]

{"sheet":"dvi_atop","index":4,"n_rows":38,"n_cols":24,"rows_kept":38,"merged":[[3,0,37,0]],"flags":["formulas_cached_only"]}
["1.表格依照開關順序排列\n2.需要delay的部分視為一個項目, python可由address來判斷該項目是否為delay\n3.SYNC_DETECT (off-line Detect)暫時未考慮",null,"統一8bits",null,"此欄位表示該reg On/off開關\n與其他reg的設定剛好相反\nex: \n一般ON=0x00, OFF=0x01, Invert =N\n特別ON=0x01, OFF=0x00, Invert =Y","SW Debug use\nY= 要設定\nN= 不設定","ATV in \n(use internal demod)","ATV in \n(use external demod)",{"$nulls":14},"SW/CAE參考","SW/CAE參考"]
[null,"Reg Name","Address","Mask","Invert","Valid","CVBSO-I","CVBSO-E","DTV-DVB","DTV-ATSC","ATV-VIF","ATV-SSIF","CVBS","RGB","SCART","YPbPr","HDMI1","HDMI2","HDMI3","HDMI4","S-Video","USB","Power consumption","Description"]
[null,"P0_PD_DVIPLL","0x1109C0","0x80","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"power down DVIPLL at P1"]
[null,"P1_PD_DVIPLL","0x1132C0","0x80","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"power down DVIPLL at P1"]
[null,"P2_PD_DVIPLL","0x1134C0","0x80","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"power down DVIPLL at P2"]
[null,"P0_PD_CLKIN","0x000e96","0x10","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"power down ONLINE clock detection at P0"]
[null,"P1_PD_CLKIN","0x000e96","0x20","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"power down ONLINE clock detection at P1"]
[null,"P2_PD_CLKIN","0x000e96","0x40","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"power down ONLINE clock detection at P2"]
[null,"P0_PD_CLKIN_OFF","0x000e95","0x10","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"power down OFFLINE clock detection at P0"]
[null,"P1_PD_CLKIN_OFF","0x000e95","0x20","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"power down OFFLINE clock detection at P1"]
[null,"P2_PD_CLKIN_OFF","0x000e95","0x40","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"power down OFFLINE clock detection at P2"]
[null,"P0_PD_IBGREX","0x000e96","0x01","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"power down DM_TOP internal current source at P0"]
[null,"P1_PD_IBGREX","0x000e96","0x02","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"power down DM_TOP internal current source at P1"]
[null,"P2_PD_IBGREX","0x000e96","0x04","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"power down DM_TOP internal current source at P2"]
[null,"P0_PD_ENVDET","0x1109BE","0x01","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"power down envelop detection at P0"]
[null,"P1_PD_ENVDET","0x1132BE","0x01","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"power down envelop detection at P1"]
[null,"P2_PD_ENVDET","0x1134BE","0x01","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"power down envelop detection at P2"]
[null,"P0_PD_DM[2:0]","0x1109C0","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"powern down preamp and demux at P0"]
[null,"P1_PD_DM[2:0]","0x1132C0","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"powern down preamp and demux at P1"]
[null,"P2_PD_DM[2:0]","0x1134C0","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"powern down preamp and demux at P2"]
[null,"P0_PD_MXD[2:0]","0x1109C1","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"power down mixer at P0"]
[null,"P1_PD_MXD[2:0]","0x1132C1","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"power down mixer at P1"]
[null,"P2_PD_MXD[2:0]","0x1134C1","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"power down mixer at P2"]
[null,"PD_RD0[2:0]","0x1109C1","0x38","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"power down the R-term of the data channel at P0"]
[null,"PD_RD1[2:0]","0x1132C1","0x38","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"power down the R-term of the data channel at P1"]
[null,"PD_RD2[2:0]","0x1134C1","0x38","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"power down the R-term of the data channel at P1"]
[null,"PD_RCK[0]","0x000e97","0x01","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"power down the R-term of the clock channel at P0"]
[null,"PD_RCK[1]","0x000e97","0x02","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"power down the R-term of the clock channel at P1"]
[null,"PD_RCK[2]","0x000e97","0x04","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"power down the R-term of the clock channel at P2"]
[null,"PD_P0_DPLPHI[2:0]","0x1109fe","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"power down the phase dac of P0 Iclk"]
[null,"PD_P1_DPLPHI[2:0]","0x1132e8","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"power down the phase dac of P1 Iclk"]
[null,"PD_P2_DPLPHI[2:0]","0x1134e8","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"power down the phase dac of P2 Iclk"]
[null,"PD_P0_DPLPHQ[2:0]","0x1109fe","0x38","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"power down the phase dac of P0 Qclk"]
[null,"PD_P1_DPLPHQ[2:0]","0x1132e8","0x38","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"power down the phase dac of P1 Qclk"]
[null,"PD_P2_DPLPHQ[2:0]","0x1134e8","0x38","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"power down the phase dac of P2 Qclk"]
[null,"ARC0_OEN","0x101a2a","0x02","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF","OFF",null,"output enable of the audio return channel at P0, active low"]
[null,"ARC1_OEN","0x101a2a","0x10","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF","OFF",null,"output enable of the audio return channel at P1, active low"]
[null,"ARC2_OEN","0x101a2a","0x80","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF",null,"output enable of the audio return channel at P2, active low"]

{"sheet":"dvi_top_oneport","index":5,"n_rows":16,"n_cols":24,"rows_kept":16,"merged":[[2,0,15,0]],"flags":["formulas_cached_only"]}
["1.表格依照開關順序排列\n2.需要delay的部分視為一個項目, python可由address來判斷該項目是否為delay\n3.SYNC_DETECT (off-line Detect)暫時未考慮",null,"統一8bits",null,"此欄位表示該reg On/off開關\n與其他reg的設定剛好相反\nex: \n一般ON=0x00, OFF=0x01, Invert =N\n特別ON=0x01, OFF=0x00, Invert =Y","SW Debug use\nY= 要設定\nN= 不設定","ATV in \n(use internal demod)","ATV in \n(use external demod)",{"$nulls":14},"SW/CAE參考","SW/CAE參考"]
[null,"Reg Name","Address","Mask","Invert","Valid","CVBSO-I","CVBSO-E","DTV-DVB","DTV-ATSC","ATV-VIF","ATV-SSIF","CVBS","RGB","SCART","YPbPr","HDMI1","HDMI2","HDMI3","HDMI4","S-Video","USB","Power consumption","Description"]
["DVI_TOP_ONEPORT","P0_PD_BG","0x000e97","0x80","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down internal BG at P3"]
[null,"P0_PD_REG","0x1109d2","0x20","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down DVIPLL REG at P3"]
[null,"P0_PD_DVIPLL","0x1109d2","0x80","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down DVIPLL at P3"]
[null,"P0_PD_CLKIN","0x000e96","0x80","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down ONLINE clock detection at P3"]
[null,"P0_PD_CLKIN_OFF","0x000e95","0x80","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down OFFLINE clock detection at P3"]
[null,"P0_PD_IBGREX","0x000e96","0x08","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down DM_TOP internal current source at P3"]
[null,"P0_PD_ENVDET","0x1109d8","0x01","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down envelop detection at P3"]
[null,"P0_PD_DM[2:0]","0x1109d2","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"powern down preamp and demux at P3"]
[null,"P0_PD_MXD[2:0]","0x1109d3","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down mixer at P3"]
[null,"PD_RD0[2:0]","0x1109d3","0x38","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down the R-term of the data channel at P3"]
[null,"PD_RCK","0x000e97","0x08","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down the R-term of the clock channel at P3"]
[null,"PD_P0_DPLPHI[2:0]","0x1109ff","0x07","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down the phase dac of P3 Iclk"]
[null,"PD_P0_DPLPHQ[2:0]","0x1109ff","0x38","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"power down the phase dac of P3 qclk"]
[null,"ARC0_OEN","0x101a2b","0x04","N","N","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","OFF","ON","OFF","OFF","OFF",null,"output enable of the audio return channel at P3, active low"]