{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["工作表1","工作表2","工作表3"],"read":"whole","date_system":"1900"}

{"sheet":"工作表1","index":0,"n_rows":182,"n_cols":6,"rows_kept":182}
["API Version ","Date","Submitter","Project Name","Descripition","Compatibility(Y/N)"]
[1,"2014-05-27","River.Cheng","R_Utopia2__main","refine CH34/GOPSCD/DAC/ACP header file \n(move OPEN/CLOSE/IOCTL from API_v2.h to API_private.h)","Y"]
[2,"2014-05-27","Carlos.Tsai","R_Utopia2__main","Add an API (MDrv_AESDMA_IsSecretKeyInNormalBank())","Y"]
[3,"2014-05-27","yc.wang","R_Utopia2__main","Add an API to get DRAM size (MDrv_MIU_Dram_ReadSize)","Y"]
[4,"2014-05-28","Dixon.Wang","R_Utopia2__main","Add a enum for the new MOD interface EPI28_12P"]
[5,"2014-05-28","Matt.Sung","R_Utopia2__main","Add enum for Monaco SYS PAD config","Y"]
[6,"2014-05-27","yc.wang","R_Utopia2__main","Add an API to get DRAM size (MDrv_MIU_Dram_ReadSize)","Y"]
[7,"2014-05-28","yc.wang","R_Utopia2__main","Add utopia2 code in MIU, so add include header file drvMIU_v2.h in drvmiu.h","Y"]
[8,"2014-05-30","Dixon.Wang","R_Utopia2__main","Add the definition of DBG level ","Y"]
[9,"2014-05-30","Carlos.Tsai","R_Utopia2__main","Add an API to set HDCP","Y"]
[10,"2014-06-04","yc.wang","R_Utopia2__main","Move cmd id to drvbdma_v2.h","Y"]
[11,"2014-06-04","Doyle.Huang","R_Utopia2__main","Add an API to get SAR KeyValue with every SAR Channel","Y"]
[12,"2014-06-04","Dixon.Wang","R_Utopia2__main","change the ldHz in drvPNL.h from U32 to U64 for 600MHz\n** drvPNL.h is not public header"]
[13,"2014-06-05","Dixon.Wang","R_Utopia2__main","remove some drv header files from the public header folder"]
[14,"2014-06-05","Johnny.Ko","R_Utopia2__main","Add a new get control command to get HW MAX PIXEL of decoder","Y"]
[15,"2014-06-05","Jonathan.Yen","R_Utopia2__main","add new LPLL type for Miami","Y"]
[16,"2014-06-06","Timothy.Lee","R_Utopia2__main","Refine exception","Y"]
[17,null,null,"R_Utopia2__main","Add \"DMX_FLOW_PLAYBACK_FI\" to \"DMX_FLOW\" enum for new HW","Y"]
[18,"2014-06-06","Namodtum.Lu","R_Utopia2__main","Add enum for MIU client","Y"]
[19,"2014-06-10","Marius.Wang","R_Utopia2__main","Add enum for Audio MM Type","Y"]
[20,"2014-06-11","dirk.hu","R_Utopia2__main","Add E_XC_SUPPORT_FRCM_MODE for E_XC_CAPS to decide if need set frcm address","Y"]
[21,"2014-06-11","Jeff.Shen","R_Utopia2__main","Add MDrv_USB_Port_Close()  and MDrv_USB_MscLookupVidPid()","Y"]
[22,"2014-06-12","Peifen.chen","R_Utopia2__main","Add MApi_GOP_GWIN_DeleteWinHVSize for Delete unexpect out HV size.(But users wants reference data when streching.)","Y"]
[23,"2014-06-16","Peifen.chen","R_Utopia2__main","Remove unused enum items.","Y"]
[24,"2014-06-16","jeffrey.su","R_Utopia2__main","Add disable AVS+ parser function for psuedo start code issue"]
[25,"2014-06-17","joe.liu","R_Utopia2__main","Add ION API","Y"]
[26,"2014-06-17","Ives.Chen","R_Utopia2__main","Add CH34 new mode"]
[27,"2014-06-19","Jeff.Shen","R_Utopia2__main","Refine local definition","Y"]
[28,"2014-06-20","River.Cheng","R_Utopia2__main","Sync apiXC_EX header from utopia CL855707 and sync struct because of struct in apiXC.h has changed","N (This CL is for K3S only.)"]
[29,"2014-06-20","CJ.hsu","R_Utopia2__main","Add enum for Supernova add msdk","Y"]
[30,"2014-06-23","Harold.Chen","R_Utopia2__main","add apiVDEC_MultiDec.h for vdec3.0","N(It is the first release for Vdec3.0)"]
[31,"2014-06-24","Lester.Lee","R_Utopia2__main","Add enum for set play rate API for WIDI","Y"]
[32,"2014-06-25","Namodtum.Lu","R_Utopia2__main","Add enum for seal client","Y"]
[33,"2014-06-25","Apple.Chen","R_Utopia2__main","Add VP9 setting foe Monaco","Y"]
[34,"2014-06-25","joe.liu","R_Utopia2__main","ADD:\n1. MDrv_CMDQ_Set_MIU_SELECT: MIU Setting for CMDQ_Buffer\n2. MDrv_CMDQ_Gen_WaitTrigger_Bus_Command: Gen Wait Command\n\nModify:\n1. MDrv_CMDQ_Get_Memory_Size: for supporting MIU1","Y"]
[35,"2014-06-27","chunwei.chen","R_Utopia2__main","ADD:\n1. E_XC_ADC_CMD_SET_IDACCURRENTMODE: psXCInstPri->fpXC_ADC_SetIdacCurrentMode\n2. E_XC_ADC_CMD_GET_IDACCURRENTMODE: psXCInstPri->fpXC_ADC_GetIdacCurrentMode","Y"]
[36,"2014-06-27","Elle.Ko","R_Utopia2__main","Add enum for Sync STC in MM TS file","Y"]
[37,"2014-06-27","fannie.tsai","R_Utopia2__main","Add enum for new dscmb HW","Y"]
[38,"2014-06-28","jamie.lien","R_Utopia2__main","Add new API for read/write OTP field","Y"]
[39,"2014-06-30","Matt.Sung","R_Utopia2__main","Revert 892087 requested by Joe.Liu","Y"]
[40,"2014-06-30","Art.Huang","R_Utopia2__main","Add 3D frame packing and 4K2K output timing","Y"]
[41,"2014-06-30","Timothy.Lee","R_Utopia2__main","Sync Utopia Cipher driver CL#878865","Y"]
[42,"2014-06-30","fannie.tsai","R_Utopia2__main","1. Add DMX_QUERY_TYPE enum\n2. Add DMX_TEI_RmPktType (sync form api/apiDMX.h)","Y"]
[43,"2014-07-01","dirk.hu","R_Utopia2__main","Add E_PQ_IOCTL_PQ_SUGGESTED_FRCMFRAMENUM enum for PQ to set frcm frame number","Y"]
[44,"2014-07-02","Johnny.Ko","R_Utopia2__main","add new command VDEC_USER_CMD_GET_DS_BUF_MIU_SEL for vdec 1.0 inerface wrapper","Y"]
[45,"2014-07-02","Albert-PT.Lin","R_Utopia2__main","Add 4K2K output timing","Y"]
[46,"2014-07-03","chunwei.chen","R_Utopia2__main","add  instant  for drv use","Y"]
[47,"2014-07-03","Dixon.Wang","R_Utopia2__main","Add new parameters for Vbox Information \nsync from UTPA2-201.0.x_Napoli for 4K2K DS solution"]
[48,"2014-07-03","Richard.Ni","R_Utopia2__main","Add new enum INTERNAL_ATVENC for AUDIO_INTERNAL_PATH_TYPE","Y"]
[49,"2014-07-03","chunwei.chen","R_Utopia2__main","add extern to avoid miltiple include","Y"]
[50,"2014-07-04","fannie.tsai","R_Utopia2__main","1. Remove TSO VQ buffer parameters form DMX_TSPParam structure\n2. Add MApi_DMX_TSO_SVQBuf_Set API for setting TSO VQ buffer ","N\nY"]
[51,"2014-07-04","Desmond.Pu","R_Utopia2__main","Add new api for Fastboot\nIn Mboot of Fastboot, Utopia Init is not neccesary, so remove it from MsOS_Init","Y"]
[52,"2014-07-07","River.Cheng","R_Utopia2__main","to sync apiPNL.h in utopia1.0, add #include \"MsVersion.h\" to apiPNL.h","Y"]
[53,"2014-07-07","fannie.tsai","R_Utopia2__main","1. Add mew enum itiemto DMX_QUERY_TYPE\n2. Modify MApi_DMX_TSO_LocalStreamId API interface\n3. Add DMX_TSO_InputIf , new enum\n4. Add new API, MApi_DMX_MStr_SrcIdSyncByte\n5. Modify DMX_TSO_LOCSTRID_PARAM structure\n6. Add enum values to eDmxIoctlOpt\n7. Add new structure, DMX_MSTR_SRCID_SYNCBY_PARAM\n8. Add enum item E_DRVTSO_OUTCLK_27M to DrvTSO_OutClk","Y\nY\nN: But no one use it yet.\nY\nN: But no one use it yet.\nY\nY\nY"]
[54,"2014-07-07","Zhi Zhan Chen","R_Utopia2__main","Add vdec HW capability for upper layer query.","Y"]
[55,"2014-07-07","Namodtum.Lu","R_Utopia2__main","add aarch64 compile environment","Y"]
[56,"2014-07-08","Nathan.Kao","R_Utopia2__main","add GE TLB API","Y"]
[57,"2014-07-08","Jonathan.Yen","R_Utopia2__main","add E_XC_SUPPORT_INTERLACE_OUT enum in E_XC_CAPS","Y"]
[58,"2014-07-08","Dixon.Wang","R_Utopia2__main","1. add enum MS_HDMI_COLOR_YUV_420 for HDMI2.0 spec\n2. add MDrv_HDMI_CheckHDMI20_Setting to check the input pixel pixel rate and setup the HDMI from 1P to 2P"]
[59,"2014-07-09","joe.liu","R_Utopia2__main","1. Add define for command_type\n2. add one parameter for MDrv_CMDQ_Init to set CMDQ_BUFFER_MIU_SELECT\n3. change parameter of MDrv_CMDQ_Gen_WaitTrigger_Bus_Command to a enum, for easier usage","Y"]
[60,"2014-07-09","Nathan.Kao","R_Utopia2__main","add a new enum(E_GOP_CAP_STRETCH) in EN_GOP_CAPS","Y"]
[61,"2014-07-09","Zhi Zhan Chen","R_Utopia2__main","Add vdec HW capability for upper layer query.","Y"]
[62,"2014-07-10","Timothy.Lee","R_Utopia2__main","Sync AESDMA API from Utopia Cipher driver","Y"]
[63,"2014-07-10","Chalrie.Chen","R_Utopia2__main","Add VP9 enum in apiVDEC.h","Y"]
[64,"2014-07-10","Leon.Zhao","R_Utopia2__main","Add MApi_XC_Combine_MLoadEn, remove MApi_XC_Set_Zorder_MLoadEn","N: But no one use it yet."]
[65,"2014-07-10","ian-hy.lin","R_Utopia2__main","Add new API MDrv_SYS_GetIpList for get this chip IP List","Y"]
[66,"2014-07-10","cy.lai","R_Utopia2__main","Add mfe HW capability for upper layer query.","Y"]
[67,"2014-07-11","apple.Chen","R_Utopia2__main","Add enum 320MHz to MVOP_FREQUENCY for clippers","Y"]
[68,"2014-07-14","Nathan.Kao","R_Utopia2__main","add a value in the strutrue of GOP_CAP_STRETCH_INFO .  To extend GOP stretch info","Y"]
[69,"2014-07-14","Nathan.Kao","R_Utopia2__main","delete useless gop stretch data in the strutrue of GOP_CAP_STRETCH_INFO.","N: But no one use it yet."]
[70,"2014-07-15","Apple.Chen","R_Utopia2__main","Add Enum 72MHz and 108 MHz to MVOP_FREQUENCY for Keres","Y"]
[71,"2014-07-16","Peifen.chen","R_Utopia2__main","Add enum for get maxim FB number."]
[72,"2014-07-17","fannie.tsai","R_Utopia2__main","1. Refine MApi_DMX_MStr_SyncByte\n2. Add new commends to 2.0 IO control\n3. Add new enum items to DMX_FILTER_TYPE","1. N: But no one use it yet.\n2. Y\n3. Y"]
[73,"2014-07-18","Art.Huang","R_Utopia2__main","In 4K2K output timing, panel H back porch value will overflow (type is U8).\nAnd panel H start value will be wrong if H back porch overflowed.\nTherefore add a function to force setting panel H start to the correct value.","Y"]
[74,"2014-07-18","Point.Huang","R_Utopia2__main","Add Enum to APIPNL_LINK_EXT_TYPE for Madison bypass mode","Y"]
[75,"2014-07-18","Jway.Lin","R_Utopia2__main","Add new interface & struct for Utopia2k ","Y"]
[76,"2014-07-21","Chei.Lin","R_Utopia2__main","Sync to utopia main trunk and ATSC supports STR.","Y"]
[77,"2014-07-21","Erdenebat.Ul","R_Utopia2__main","NSK2, EMM new driver for Keres HW test/Harm","Y"]
[78,"2014-07-22","Leon.Zhao","R_Utopia2__main","1.support multi gop update once;\n2.support multi alpha."]
[79,"2014-07-24","Carlos.Tsai","R_Utopia2__main","1. Refine API when using HW Parser start. 2. It will not execute sw reset if cipher engine is CTR","Y"]
[80,"2014-07-24","Doyle.Huang","R_Utopia2__main","Refine SEAL Enum for driver usage"]
[81,"2014-07-24","joe.Liu","R_Utopia2__main","Add ION API","Y"]
[82,"2014-07-24","Doyle.Huang","R_Utopia2__main","Refine MSIRQ total interrupt number","Y"]
[83,"2014-07-25","fannie.tsai","R_Utopia2__main","Update DMX_FILTER_FLT_MASK definie value for new setting","Y"]
[84,"2014-07-25","dirk.hu","R_Utopia2__main","add E_XC_SUPPORT_4K2K_WITH_PIP for support 4k2k with pip","Y"]
[85,"2014-07-25","wilson.hsu","R_Utopia2__main","Add Audio_Comm_infoType_Set_DFS_PowerSave for R2/DSP Fs control","Y"]
[86,"2014-07-25","Apple.Chen","R_Utopia2__main","Add new structure MVOP_GetMaxFps for E_MVOP_CMD_GET_MAX_FPS","Y"]
[87,"2014-07-25","Peter.Wu","R_Utopia2__main","Add Utopia2K - HWI2C","Y"]
[88,null,null,"R_Utopia2__main","Add Armv8 define flag","Y"]
[89,"2014-07-28","joe.liu","R_Utopia2__main","add missed API","Y"]
[90,"2014-07-29","Cindy.Chiu","R_Utopia2__main","add enum E_AVI_INFOFRAME_VERSION3 for HDMI2.0 spec","Y"]
[91,"2014-07-29","Jonathan.Yen","R_Utopia2__main","MS_BOOL MApi_PNL_GetOutputInterlaceTiming(void)","Y"]
[92,"2014-07-30","fannie.tsai","R_Utopia2__main","1. Modify DMX_FlowInput_Info parameters\n2. Add new items to DMX_QUERY_TYPE\n3. Add TSO new data structure & APIs\n4. Add new items to eDmxIoctlOpt","1. N : But no one use it yet\n2. Y\n3. Y\n4. Y"]
[93,"2014-07-31","Dixon.Wang","R_Utopia2__main","add new mux output for SC2","N : But no one use it yet"]
[94,"2014-08-01","Wilson.Chang","R_Utopia2__main","adding functions for HDCP22","Y"]
[95,"2014-08-01","Nancy.Lin","R_Utopia2__main","Add enum for get brightness for backward compatibility with Utopia v1.0","Y"]
[96,"2014-08-01","joe.liu","R_Utopia2__main","Refine CMDQ","Y"]
[97,"2014-08-04","joe.liu","R_Utopia2__main","Add #include \"MsTypes.h\" to drvCMDQ.h","Y"]
[98,"2014-08-04","Albert-PT.Lin","R_Utopia2__main","add new enum for HDMITx","Y"]
[99,"2014-08-04","Carlos.Tsai","R_Utopia2__main","Refine the HDCP22 API for Monaco","Y"]
[100,"2014-08-04","Nathan.Kao","R_Utopia2__main","1. add set GOP TLB API\n2. add set GOP GPUtile mode API\n3. add supoort GOP TLB enum in GOP capacity struct","Y"]
[101,"2014-08-05","fannie.tsai","R_Utopia2__main","Add new IO control commends","Y"]
[102,"2014-08-05","Wilson.Chang","R_Utopia2__main","1. adding power state function for HDMI tx to restore HDMI tx settings when exit PM mode","Y"]
[103,"2014-08-05","darren.chen","R_Utopia2__main","Support to get DSP1 & DSP2's AV Sync Offset.","Y"]
[104,"2014-08-06","wanting.huang","R_Utopia2__main","Add an OPCapture Blending point to select capturing from the last OSD Blend.","Y"]
[105,"2014-08-06","yiikai.wang","R_Utopia2__main","1. add API to set CC SC window length\n2. add API to set CC video standard\n3. refine eVBIIoctlOpt enum","Y\nY\nN: But no one use it yet."]
[106,"2014-08-06","jacky.chang","R_Utopia2__main","add multiple frame header enum","Y"]
[107,"2014-08-07","sam.hsu","R_Utopia2__main","add apiGOP_priv.h for private struct and enum","Y"]
[108,"2014-08-07","fannie.tsai","R_Utopia2__main","Add MApi_DMX_MMFI_TimeStampClk","Y"]
[109,"2014-08-07","Leon.Zhao","R_Utopia2__main","Add MApi_GOP_GWIN_GetLayer\nMApi_GOP_GWIN_GetLayerFromGOP\nMApi_GOP_GWIN_GetGOPFromLayer","Y"]
[null,null,"Peifen.chen","R_Utopia2__main","Implement symbol  DLL_LOCAL/DLL_PUBLIC\napiGOP.h\napiGFX.h\napiXC_DWIN.h ","Y"]
[111,"2014-08-13","Jesse.Chou","R_Utopia2__main","Add PQ_XC_ID enum","Y"]
[112,"2014-08-13","Chei.Lin","R_Utopia2__main","Update drvDMD_ATSC.h. \nSupport utopia2.0 and multi-demod.","N\nIt is the 1st release."]
[113,"2014-08-14","Chienfong.huang","R_Utopia2__main","Add HBBTV query Enum to drvSYS.h","Y"]
[114,"2014-08-14","Chei.Lin","R_Utopia2__main","Sync drvDMD_DTMB.h to utopia main.","Y"]
[115,"2014-08-15","CJ.hsu","R_Utopia2__main","Add enum for DTS-HD/Dolby TrueHD bypass","Y"]
[116,"2014-08-15","Jesse.chou","R_Utopia2__main","Add PQ EX call back APIs.","Y"]
[117,"2014-08-15","Charlie.Wu","R_Utopia2__main","Add include Mstypes.h in Apivdec.h","Y"]
[118,"2014-08-15","Dixon.Wang","R_Utopia2__main","modify the enum of E_MUX_OUTPUTPORT and E_DEST_TYPE, original setting is not correct","N: But no one use it yet."]
[119,"2014-08-16","Dixon.Wang","R_Utopia2__main","add a new function for SC2 VOP timing setting","N: But no one use it yet."]
[120,"2014-08-18","Sam.hsu","R_Utopia2__main","add SCALER_DIP_SOURCE_TYPE_SC2_OP_CAPTURE"]
[121,"2014-08-21","Chei.Lin","R_Utopia2__main","add the driver function of MDrv_DMD_ATSC_SetReset and MDrv_DMD_ATSC_MD_SetReset.","Y"]
[122,"2014-08-22","chunwei.chen","R_Utopia2__main","add new ioctl function for g_Ipanel"]
[123,"2014-08-22","Dianetics.kao","R_Utopia2__main","add Hal_HDMI_StablePolling function for HDMI 2.0 polling event handler","Y"]
[124,"2014-08-24","Szuhua.Wu","R_Utopia2__main","add new API  MApi_XC_Is_SupportSWDS / MApi_XC_GetSWDSIndex","Y"]
[125,"2014-08-26","Dianetics.kao","R_Utopia2__main","add Hal_HDMI_GetSourceVersionType function for check source support HDMI 2.0 or not","Y"]
[126,"2014-08-27","Roger.He","R_Utopia2__main","add new API for cma pool","N: But no one use it yet."]
[127,"2014-08-27","yc.wang","R_Utopia2__main","Add emu for on chip 8024 smart card mode"]
[128,"2014-08-29","Chei.Lin","R_Utopia2__main","add the driver function of MDrv_DMD_ATSC_SEL_DMD, MDrv_DMD_ATSC_SetVsbMode, MDrv_DMD_ATSC_Set256QAMMode and MDrv_DMD_ATSC_Set64QAMMode to fix compile error.","Y"]
[129,"2014-09-03","Cindy.Chiu","R_Utopia2__main","add CEC port select API","Y"]
[130,"2014-09-04","Leon.Zhao","R_Utopia2__main","add enum member to E_XC_OSD_INDEX","N: But no one use the member yet."]
[131,"2014-09-04","Erin.Yang","R_Utopia2__main","Add MApi_VDEC_EX_SetFrmBuff2() for the second frame buffer","N: But no one use the member yet."]
[132,"2014-09-04","yiikai.wang","R_Utopia2__main","sync API MDrv_SYS_SetTSClockPhase from utopia1.0","Y"]
[133,"2014-09-04","fannie.tsai","R_Utopia2__main","1. DMX_TSPParam - add \"u32Res\",  change \"_zero_reserved[3] to be _zero_reserved[2]\n2. Add \"u32Res\" to DMX_TSO_InputCfg/DMX_TSO_OutputCfg structures\n3. Add \"u32Res\" to sturctures of apiDMX_v2.h","1. N: 若有使用_zero_reserved,會不相容\n2. N : TSO 功能CI team 開發中,尚未release,所以不影響\n3. N: 目前上層都是call 1.0 API, 2.0 API 只有driver 內部使用,所以不影響"]
[134,"2014-09-10","Jeff.Shen","R_Utopia2__main","Add new API","Y"]
[135,"2014-09-10","sam.hsu","R_Utopia2__main","Add new enum DIP_DATA_FMT_YUV420_PLANER and DIP_DATA_FMT_YUV420_SEMI_PLANER","Y"]
[136,"2014-09-11","sam.hsu","R_Utopia2__main","Add new enum E_GOP_SEL_MIU2 and E_GOP_SEL_MIU3","Y"]
[137,"2014-09-11","Peifen.chen","R_Utopia2__main","Using weak symbol for symbol release.","Y"]
[138,"2014-09-12","ajay.liu","R_Utopia2__main","[Audio] Sync Enum with mapi_audio_datatype.h","Y"]
[139,"2014-09-13","ken.chang","R_Utopia2__main","add #define SYMBOL_WEAK __attribute__((weak))","Y"]
[140,"2014-09-24","Wilson.Hsu","UTPA2-204.0.x_Monaco","add Enum  for  getting IC use R2/DSP decode","Y"]
[141,"2014-09-25","Dianetics.kao","UTPA2-204.0.x_Monaco","add MDrv_HDMI_Set5VDetectGPIOSelect to select 5V detect GPIO","Y"]
[142,"2014-10-08","Yd.tsai","utopia2_Muji","Update drvDMD_DTMB.h. \nSupport utopia2.0 and multi-demod.","N\nIt is the 1st release."]
[143,"2014-10-24","Chei.lin","utopia2_Muji","Suport STR function","N\nIt is the 1st release."]
[144,"2014-10-27","Wright.Huang","utopia2_Muji","1. add ACE API to set ICC/IBC value.\n2. add ACE enum for ICC/IBC color","Y"]
[145,"2014-11-18","Ken-KH.Lin","utopia2_Muji","1. move mfe_ex public headers to mxlib/include (apiVOIPMFE.h, api_mfe_frmformat.h, drv_mfe_st.h)\n2. remove out-dated header from mxlib/include (drvMFE.h)","Y"]
[146,"2014-11-19","Joe.Liu","utopia2_Muji","1. move drvCMAPool.h to mxlib/include","Y"]
[147,"2014-11-19","Marcos.Ho","utopia2_Muji","Add OSD 4K1K selections","Y"]
[148,"2014-12-12","Wilson.Chang","utopia2_Muji","adding fill cipher key function to REE enviroment for HDCP22","Y"]
[149,"2014-12-13","Dixon.Wang","utopia2_Muji","make Vby1 freeswap configurable","N\nnew feature \nthe share memory size is changed. \nIt need to sync lib and header file and compiler all"]
[150,"2014-12-15","joe.liu","utopia2_Muji","Move CMA ID ENUM to public header","Y"]
[151,"2014-12-18","Point.Huang","utopia2_Muji","Add new API for pixel shift feature ( sync CL 989583 )","Y"]
[152,"2014-12-18","li.zhu","utopia3_Muji","add local dimming module:\n1. add api called by mboot:MS_U16 MApi_LD_Init(pstLD_Init_Parameters pstLDArgs, MS_U16 u16DataLen)\n2. add struct stLD_Init_Parameters","Y"]
[153,"2015-01-08","Wright.Huang","utopia2L","add MApi_XC_SetCMAHeapID","Y"]
[154,"2015-01-08","Marcos.ho","UTPA2-205.0.x_MUJI","add new PNL API :  Mapi_PNL_CheckVBY1HandshakeStatus() ","Y"]
[155,"2014-10-29","Marcos.ho","R_Utopia2__main","for RR 1450 Pixel Shift\n1. remove MApi_XC_EnablePixelShift ( )\n2. remove MApi_XC_SetPixelShiftParameters ( ) \n3. add MApi_XC_SetPixelShiftFeatures( )","Y"]
[156,"2015-01-12","starlet.fan","utopia2_Muji","Merge VBI header from Monaco","Y"]
[157,"2015-01-13","Marcos.ho","utopia2_Muji","revert __aarch64__","Y"]
[158,"2015-01-14","Dianetics.kao","utopia2_Muji","Add mapi_mhl_GetExtendDeviceCapacibility function","Y"]
[159,"2015-01-15","Carlos.Tsai","utopia2_Muji","Add new API MDrv_HDCP_GetHdcpCipherState","Y"]
[160,"2015-01-16","marvin.chen ","utopia2_Muji","support Frame packing 640X480P","Y"]
[161,"2015-01-19","Point.Huang","utopia2_Muji","add enum for pixel shift","Y"]
[162,"2015-01-20","Leon.Huang","utopia2_Muji","Add MApi_XC_Get_FRCM_W_BaseAddr","Y"]
[163,"2015-01-22","Szuhua.Wu","utopia2_Muji","Add  structure member of  XC_ApiStatusEx","Y"]
[164,"2015-02-16","apple.Chen","utopia2_Monet","Add new command: E_MVOP_CMD_SET_HANDSHAKE_MODE/E_MVOP_CMD_SET_FRC_OUTPUT/E_MVOP_CMD_GET_CROP_FOR_XC","Y"]
[165,"2015-02-17","Johnny.Ko","utopia2_Muji","add new command by syncing vdec related header file","Y"]
[166,"2015-02-26","Carlos.Tsai","utopia2_Muji","add 2 enums for MIU Client Table","Y"]
[167,"2015-03-04","York.Chiu","utopia2_Muji","merge code from #cl985052","Y"]
[168,"2015-03-02","Harold.Chen","utopia2_Muji","Add E_VDEC_EX_USER_CMD_GET_NEXT_DISP_FRAME_INFO_EXT,\nE_VDEC_EX_USER_CMD_GET_VSYNC_BRIDGE_EXT_ADDR, \nE_VDEC_EX_USER_CMD_MFCODEC_MODE\ncmd","N\nIt is the 1st release."]
[169,"2015-03-16","marius.wang","utopia2_Muji","add MApi_AUDIO_DigitalOut_SetDeviceCapability and about enum","y"]
[170,"2015-03-24","dirk.hu","utopia2_Muji","add E_XC_INIT_MISC_A_SAVE_MEM_MODE in XC_INIT_MISC_A","y"]
[171,"2015-03-24","richard.deng","utopia2_Monet","add MApi_XC_SetBwdConfig","y"]
[172,"2015-04-09","dirk.hu","utopia2_muji","add MApi_XC_ConfigCMA","y"]
[173,"2015-04-30","Carlos.Tsai","UTPA2-204.0.x_Monaco","Add an Enum for querying Secured IC,  \"E_SYS_QUERY_SECURED_IC_SUPPORTED\"","Y"]
[174,"2015-05-08","Terry.Huang","utopia2_muji","Add enum value for TSO new functions","Y"]
[175,"2015-05-27","yiikai.wang","utopia2_muji","1. add API MDrv_DSCMB2_HDCP2_SetRIV_Ex to compatible with STB\n2. add enum E_DSCMB_FLT_1_KEYS to compatible with STB","Y"]
[176,"2015-06-03","Terry.Huang","utopia2_muji","Add TSO new functions","Y"]
[177,"2015-06-17","Tom.Liu","UTPA2-500.0.x","1. combine hashkey flow\n2. use AUDIO_SHARED_VARS2 to decide dd encoder spdif mode","Y"]
[178,"2015-07-06","leon.zhao","UTPA2-500.0.x","add enum E_XC_SUPPORT_PIP_PATCH_USING_SC1_MAIN_AS_SC0_SUB","Y"]
[179,"2015-07-13","ken-kh.lin","UTPA2-500.0.x","Add define \"MFE_SUPPORT_REDUCE_MODE\" in \"drv_mfe_st.h\".","Y"]
[180,"2015-07-17","leon.zhao","UTPA2-500.0.x","Add enum member E_VIDEO_ON_OSD_LAYER_4 to E_VIDEO_ON_OSD_LAYER","Y"]
[181,"2015-07-20","sofa.xie","UTPA2-500.0.x","Add xc test pattern api","Y"]

{"sheet":"工作表2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"工作表3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}